Additional Topics > Medical Imaging in IDL > DICOM Resources > DICOM Attributes

# DICOM Attributes

A DICOM attribute or data element is composed of the following parts:

- A tag, in the format of group, element (`XXXX`,`XXXX`) that identifies the element
- A Value Representation (VR) that describes the data type and format of the attribute’s value
- A value length that defines the length of the attribute’s value
- A value field containing the attribute’s data

The basic attribute structure is shown in the following figure:

Each data element is described by a pair of numbers (group number, data element number). Even numbered groups are elements defined by the DICOM standard and are referred to as public tags. Odd numbered groups can be defined by users of the file format, but must conform to the same structure as standard elements. These are referred to as private tags.

Note: This section does not contain a comprehensive IOD list for each modality. Visit http://medical.nema.org/dicom.html for additional DICOM information including access to the complete standard.

The following table lists the DICOM attributes organized by attribute name. This information comes from the 2001 NEMA DICOM Standard (http://medical.nema.org/dicom/2001.html). See Value Representations for definitions of the VR items.

To search for an attribute, click in the table, press Ctrl + F, enter the text or number, and click Find Next. Or, search the attribute name by letter:

A | B | C | D | E | F | G | H | I | K | L | M | N | O | P | Q | R | S | T | U | V | W | X | Y | Z

Attribute Name | VR | Tag
Accession Number | SH | (0008,0050)
Acquisition Context Description | ST | (0040,0556)
Acquisition Context Sequence | SQ | (0040,0555)
Acquisition Date | DA | (0008,0022)
Acquisition Datetime | DT | (0008,002A)
Acquisition Device Processing Code | LO | (0018,1401)
Acquisition Device Processing Description | LO | (0018,1400)
Acquisition Matrix | US | (0018,1310)
Acquisition Number | IS | (0020,0012)
Acquisition Start Condition | CS | (0018,0073)
Acquisition Start Condition Data | IS | (0018,0074)
Acquisition Termination Condition | CS | (0018,0071)
Acquisition Termination Condition Data | IS | (0018,0075)
Acquisition Time | TM | (0008,0032)
Acquisition Time Synchronized | CS | (0018,1800)
Acquisitions in Study | IS | (0020,1004)
Active Source Diameter | DS | (300A,0218)
Active Source Length | DS | (300A,021A)
Actual Frame Duration | IS | (0018,1242)
Actual Human Performers Sequence | SQ | (0040,4035)
Additional Drug Sequence | SQ | (0018,002A)
Additional Patient History | LT | (0010,21B0)
Administration Route Code Sequence | SQ | (0054,0302)
Admission ID | LO | (0038,0010)
Admitting Date | DA | (0038,0020)
Admitting Diagnoses Code Sequence | SQ | (0008,1084)
Admitting Diagnoses Description | LO | (0008,1080)
Admitting Time | TM | (0038,0021)
Air Kerma Rate Reference Date | DA | (300A,022C)
Air Kerma Rate Reference Time | TM | (300A,022E)
Anatomic Region Modifier Sequence | SQ | (0008,2220)
Anatomic Region Sequence | SQ | (0008,2218)
Anatomic Structure, Space or Region Sequence | SQ | (0008,2229)
Anchor Point | FL | (0070,0014)
Anchor Point Annotation Units | CS | (0070,0004)
Anchor Point Visibility | CS | (0070,0015)
Angio Flag | CS | (0018,0025)
Angular Position | DS | (0018,1141)
Angular Step | DS | (0018,1144)
Angular View Vector | US | (0054,0090)
Annotation Content Sequence | SQ | (2130,0050)
Annotation Display Format ID | CS | (2010,0030)
Annotation Flag | CS | (2000,0065)
Annotation Group Number | US | (0040,A180)
Annotation Position | US | (2030,0010)
Annotation Sequence | SQ | (0040,B020)
Anode Target Material | CS | (0018,1191)
Applicable Frame Range | US | (0028,6102)
Application Setup Check | CS | (3008,0116)
Application Setup Manufacturer | LO | (300A,0238)
Application Setup Name | LO | (300A,0236)
Application Setup Number | IS | (300A,0234)
Application Setup Sequence | SQ | (300A,0230)
Application Setup Type | CS | (300A,0232)
Applicator Description | LO | (300A,010A)
Applicator ID | SH | (300A,0108)
Applicator Sequence | SQ | (300A,0107)
Applicator Type | CS | (300A,0109)
Approval Status | CS | (300E,0002)
Attached Contours | IS | (3006,0049)
Attenuation Correction Method | LO | (0054,1101)
Audio Comments | LT | (50xx,200E)
Audio Sample Data | OW or OB | (50xx,200C)
Audio Sample Format | US | (50xx,2002)
Audio Type | US | (50xx,2000)
Authorization Equipment Certification Number | LO | (0100,0426)
Average Pulse Width | DS | (0018,1154)
Axial Acceptance | DS | (0054,1200)
Axial Mash | IS | (0054,1201)
Axis Labels | SH | (50xx,0040)
Axis Units | SH | (50xx,0030)
Basic Color Image Sequence | SQ | (2020,0111)
Basic Grayscale Image Sequence | SQ | (2020,0110)
Beam Description | ST | (300A,00C3)
Beam Dose | DS | (300A,0084)
Beam Dose Specification Point | DS | (300A,0082)
Beam Limiting Device Angle | DS | (300A,0120)
Beam Limiting Device Angle Tolerance | DS | (300A,0046)
Beam Limiting Device Leaf Pairs Sequence | SQ | (3008,00A0)
Beam Limiting Device Position Sequence | SQ | (300A,011A)
Beam Limiting Device Position Tolerance | DS | (300A,004A)
Beam Limiting Device Rotation Direction | CS | (300A,0121)
Beam Limiting Device Sequence | SQ | (300A,00B6)
Beam Limiting Device Tolerance Sequence | SQ | (300A,0048)
Beam Meterset | DS | (300A,0086)
Beam Name | LO | (300A,00C2)
Beam Number | IS | (300A,00C0)
Beam Sequence | SQ | (300A,00B0)
Beam Stopper Position | CS | (3008,0230)
Beam Type | CS | (300A,00C4)
Beat Rejection Flag | CS | (0018,1080)
Billing Item Sequence | SQ | (0040,0296)
Billing Procedure Step Sequence | SQ | (0040,0320)
Billing Supplies and Devices Sequence | SQ | (0040,0324)
Bi-Plane Acquisition Sequence | SQ | (0028,5000)
Bits Allocated | US | (0028,0100)
Bits Stored | US | (0028,0101)
Block Data | DS | (300A,0106)
Block Divergence | CS | (300A,00FA)
Block Name | LO | (300A,00FE)
Block Number | IS | (300A,00FC)
Block Number of Points | IS | (300A,0104)
Block Sequence | SQ | (300A,00F4)
Block Thickness | DS | (300A,0100)
Block Transmission | DS | (300A,0102)
Block Tray ID | SH | (300A,00F5)
Block Type | CS | (300A,00F8)
Blue Palette Color Lookup Table Data | OW | (0028,1203)
Blue Palette Color Lookup Table Descriptor | US or SS | (0028,1103)
Body Part Examined | CS | (0018,0015)
Body Part Thickness | DS | (0018,11A0)
Border Density | CS | (2010,0100)
Bounding Box Annotation Units | CS | (0070,0003)
Bounding Box Bottom Right Hand Corner | FL | (0070,0011)
Bounding Box Text Horizontal Justification | CS | (0070,0012)
Bounding Box Top Left Hand Corner | FL | (0070,0010)
Brachy Accessory Device ID | SH | (300A,0263)
Brachy Accessory Device Name | LO | (300A,0266)
Brachy Accessory Device Nominal Thickness | DS | (300A,026A)
Brachy Accessory Device Nominal Transmission | DS | (300A,026C)
Brachy Accessory Device Number | IS | (300A,0262)
Brachy Accessory Device Sequence | SQ | (300A,0260)
Brachy Accessory Device Type | CS | (300A,0264)
Brachy Application Setup Dose | DS | (300A,00A4)
Brachy Application Setup Dose Specification Point | DS | (300A,00A2)
Brachy Control Point Delivered Sequence | SQ | (3008,0160)
Brachy Control Point Sequence | SQ | (300A,02D0)
Brachy Referenced Dose Reference Sequence | SQ | (300C,0055)
Brachy Treatment Technique | CS | (300A,0200)
Brachy Treatment Type | CS | (300A,0202)
Branch of Service | LO | (0010,1081)
Burned In Annotation | CS | (0028,0301)
Calculated Dose Reference Description | ST | (3008,0074)
Calculated Dose Reference Dose Value | DS | (3008,0076)
Calculated Dose Reference Number | IS | (3008,0072)
Calculated Dose Reference Sequence | SQ | (3008,0070)
Calibration Data Sequence | SQ | (0054,0306)
Calibration Image | CS | (0050,0004)
Cardiac Number of Images | IS | (0018,1090)
Cassette Orientation | CS | (0018,1402)
Cassette Size | CS | (0018,1403)
Center of Circular Collimator | IS | (0018,1710)
Center of Circular Shutter | IS | (0018,1610)
Center of Rotation Offset | DS | (0018,1145)
Certificate of Signer | OB | (0400,0115)
Certificate Type | CS | (0400,0110)
Certified Timestamp | OB | (0400,0310)
Certified Timestamp Type | CS | (0400,0305)
Channel Baseline | DS | (003A,0213)
Channel Definition Sequence | SQ | (003A,0200)
Channel Derivation Description | LO | (003A,020C)
Channel Label | SH | (003A,0203)
Channel Length | DS | (300A,0284)
Channel Maximum Value | OB or OW | (5400,0112)
Channel Minimum Value | OB or OW | (5400,0110)
Channel Number | IS | (300A,0282)
Channel Offset | DS | (003A,0218)
Channel Sample Skew | DS | (003A,0215)
Channel Sensitivity | DS | (003A,0210)
Channel Sensitivity Correction Factor | DS | (003A,0212)
Channel Sensitivity Units Sequence | SQ | (003A,0211)
Channel Sequence | SQ | (300A,0280)
Channel Shield ID | SH | (300A,02B3)
Channel Shield Name | LO | (300A,02B4)
Channel Shield Nominal Thickness | DS | (300A,02B8)
Channel Shield Nominal Transmission | DS | (300A,02BA)
Channel Shield Number | IS | (300A,02B2)
Channel Shield Sequence | SQ | (300A,02B0)
Channel Source Modifiers Sequence | SQ | (003A,0209)
Channel Source Sequence | SQ | (003A,0208)
Channel Status | CS | (003A,0205)
Channel Time Skew | DS | (003A,0214)
Channel Total Time | DS | (300A,0286)
Cine Rate | IS | (0018,0040)
Code Meaning | LO | (0008,0104)
Code Set Extension Creator UID | UI | (0008,010D)
Code Set Extension Flag | CS | (0008,010B)
Code Value | SH | (0008,0100)
Coding Scheme Designator | SH | (0008,0102)
Coding Scheme Version | SH | (0008,0103)
Coincidence Window Width | DS | (0054,1210)
Collation Flag | CS | (2000,0063)
Collimator Left Vertical Edge | IS | (0018,1702)
Collimator Lower Horizontal Edge | IS | (0018,1708)
Collimator Right Vertical Edge | IS | (0018,1704)
Collimator Shape | CS | (0018,1700)
Collimator Type | CS | (0018,1181)
Collimator Upper Horizontal Edge | IS | (0018,1706)
Collimator/grid Name | SH | (0018,1180)
Color Image Printing Flag | CS | (2000,0062)
Column Angulation | CS | (0018,1450)
Columns | US | (0028,0011)
Comments on Radiation Dose | ST | (0040,0310)
Comments on the Performed Procedure Step | ST | (0040,0280)
Comments on the Scheduled Procedure Step | LT | (0040,0400)
Compensator Columns | IS | (300A,00E8)
Compensator ID | SH | (300A,00E5)
Compensator Number | IS | (300A,00E4)
Compensator Pixel Spacing | DS | (300A,00E9)
Compensator Position | DS | (300A,00EA)
Compensator Rows | IS | (300A,00E7)
Compensator Sequence | SQ | (300A,00E3)
Compensator Thickness Data | DS | (300A,00EC)
Compensator Transmission Data | DS | (300A,00EB)
Compensator Type | CS | (300A,00EE)
Completion Flag | CS | (0040,A491)
Completion Flag Description | LO | (0040,A492)
Compression Force | DS | (0018,11A2)
Concept Code Sequence | SQ | (0040,A168)
Conceptame Code Sequence | SQ | (0040,A043)
Confidentiality Code | LO | (0040,1008)
Confidentiality Constraint on Patient Data Description | LO | (0040,3001)
Configuration Information | ST | (2010,0150)
Configuration Information Description | LT | (2010,0152)
Constraint Weight | DS | (300A,0021)
Content Date | DA | (0008,0023)
Content Sequence | SQ | (0040,A730)
Content Template Sequence | SQ | (0040,A504)
Content Time | TM | (0008,0033)
Context Group Local Version | DT | (0008,0107)
Context Group Version | DT | (0008,0106)
Context Identifier | CS | (0008,010F)
Continuity Of Content | CS | (0040,A050)
Contour Data | DS | (3006,0050)
Contour Geometric Type | CS | (3006,0042)
Contour Image Sequence | SQ | (3006,0016)
Contour Number | IS | (3006,0048)
Contour Offset Vector | DS | (3006,0045)
Contour Sequence | SQ | (3006,0040)
Contour Slab Thickness | DS | (3006,0044)
Contrast Allergies | LO | (0010,2110)
Contrast Flow Duration(s) | DS | (0018,1047)
Contrast Flow Rate(s) | DS | (0018,1046)
Contrast Frame Averaging | US | (0028,6112)
Contrast/Bolus Administration Route Sequence | SQ | (0018,0014)
Contrast/Bolus Agent | LO | (0018,0010)
Contrast/Bolus Agent Sequence | SQ | (0018,0012)
Contrast/Bolus Ingredient | CS | (0018,1048)
Contrast/Bolus Ingredient Concentration | DS | (0018,1049)
Contrast/Bolus Route | LO | (0018,1040)
Contrast/Bolus Start Time | TM | (0018,1042)
Contrast/Bolus Stop Time | TM | (0018,1043)
Contrast/Bolus Total Dose | DS | (0018,1044)
Contrast/Bolus Volume | DS | (0018,1041)
Control Point 3D Position | DS | (300A,02D4)
Control Point Delivery Sequence | SQ | (3008,0040)
Control Point Index | IS | (300A,0112)
Control Point Relative Position | DS | (300A,02D2)
Control Point Sequence | SQ | (300A,0111)
Conversion Type | CS | (0008,0064)
Convolution Kernel | SH | (0018,1210)
Coordinate Start Value | US | (50xx,0112)
Coordinate Step Value | US | (50xx,0114)
Coordinate System Axis Code Sequence | SQ | (0040,08DA)
Corrected Image | CS | (0028,0051)
Count Rate | IS | (0018,1243)
Country of Residence | LO | (0010,2150)
Counts Accumulated | IS | (0018,0070)
Counts Included | CS | (0054,1400)
Counts Source | CS | (0054,1002)
Cranial Thermal Index | DS | (0018,5026)
Creation Date | DA | (2100,0040)
Creation Time | TM | (2100,0050)
Cumulative Dose Reference Coefficient | DS | (300A,010C)
Cumulative Dose to Dose Reference | DS | (3008,0052)
Cumulative Meterset Weight | DS | (300A,0134)
Cumulative Time Weight | DS | (300A,02D6)
Current Fraction Number | IS | (3008,0022)
Current Patient Location | LO | (0038,0300)
Current Requested Procedure Evidence Sequence | SQ | (0040,A375)
Current Treatment Status | CS | (3008,0200)
Curve Activation Layer | CS | (50xx,1001)
Curve Data | OW or OB | (50xx,3000)
Curve Data Descriptor | US | (50xx,0110)
Curve Date | DA | (0008,0025)
Curve Description | LO | (50xx,0022)
Curve Dimensions | US | (50xx,0005)
Curve Label | LO | (50xx,2500)
Curve Number | IS | (0020,0024)
Curve Range | SH | (50xx,0106)
Curve Time | TM | (0008,0035)
Data Collection Diameter | DS | (0018,0090)
Data Elements Signed | AT | (0400,0020)
Data Information Sequence | SQ | (0054,0063)
Data Set Trailing Padding | OB | (FFFC,FFFC)
Data Value Representation | US | (50xx,0103)
Date | DA | (0040,A121)
Date of Last Calibration | DA | (0018,1200)
Date of Last Detector Calibration | DA | (0018,700C)
Date of Secondary Capture | DA | (0018,1012)
DateTime | DT | (0040,A120)
dB/dt | DS | (0018,1318)
Dead Time Correction Flag | CS | (0054,1401)
Dead Time Factor | DS | (0054,1324)
Decay Correction | CS | (0054,1102)
Decay Factor | DS | (0054,1321)
Decimate/Crop Result | CS | (2020,00A2)
Default Magnification Type | CS | (2010,00A6)
Default Printer Resolution ID | CS | (2010,0054)
Default Smoothing Type | CS | (2010,00A8)
Delivered Channel Total Time | DS | (3008,0134)
Delivered Meterset | DS | (3008,0044)
Delivered Number of Pulses | IS | (3008,0138)
Delivered Primary Meterset | DS | (3008,0036)
Delivered Pulse Repetition Interval | DS | (3008,013C)
Delivered Secondary Meterset | DS | (3008,0037)
Delivered Treatment Time | DS | (3008,003B)
Delivery Maximum Dose | DS | (300A,0023)
Delivery Warning Dose | DS | (300A,0022)
Depth of Scan Field | IS | (0018,5050)
Derivation Description | ST | (0008,2111)
Destination AE | AE | (2100,0140)
Detector Activation Offset From Exposure | DS | (0018,7016)
Detector Active Dimension(s) | DS | (0018,7026)
Detector Active Origin | DS | (0018,7028)
Detector Active Shape | CS | (0018,7024)
Detector Active Time | DS | (0018,7014)
Detector Binning | DS | (0018,701A)
Detector Conditions Nominal Flag | CS | (0018,7000)
Detector Configuration | CS | (0018,7005)
Detector Description | LT | (0018,7006)
Detector Element Physical Size | DS | (0018,7020)
Detector Element Size | DS | (0054,1203)
Detector Element Spacing | DS | (0018,7022)
Detector ID | SH | (0018,700A)
Detector Information Sequence | SQ | (0054,0022)
Detector Lines of Response Used | LO | (0054,1104)
Detector Mode | LT | (0018,7008)
Detector Primary Angle | DS | (0018,1530)
Detector Secondary Angle | DS | (0018,1531)
Detector Temperature | DS | (0018,7001)
Detector Time Since Last Exposure | DS | (0018,7012)
Detector Type | CS | (0018,7004)
Detector Vector | US | (0054,0020)
Device Description | LO | (0050,0020)
Device Diameter | DS | (0050,0016)
Device Diameter Units | CS | (0050,0017)
Device Length | DS | (0050,0014)
Device Sequence | SQ | (0050,0010)
Device Serial Number | LO | (0018,1000)
Device Volume | DS | (0050,0018)
Diaphragm Position | DS | (3002,0034)
Digital Image Format Acquired | LO | (0018,1023)
Digital Signature DateTime | DT | (0400,0105)
Digital Signature UID | UI | (0400,0100)
Digital Signatures Sequence | SQ | (FFFA,FFFA)
Digitizing Device Transport Direction | CS | (0018,2020)
Directory Record Sequence | SQ | (0004,1220)
Directory Record Type | CS | (0004,1430)
Discharge Date | DA | (0038,0030)
Discharge Diagnosis Code Sequence | SQ | (0038,0044)
Discharge Diagnosis Description | LO | (0038,0040)
Discharge Time | TM | (0038,0032)
Display Window Label Vector | SH | (0018,2006)
Displayed Area Bottom Right Hand Corner | SL | (0070,0053)
Displayed Area Selection Sequence | SQ | (0070,005A)
Displayed Area Top Left Hand Corner | SL | (0070,0052)
Distance Source to Detector | DS | (0018,1110)
Distance Source to Entrance | DS | (0040,0306)
Distance Source to Patient | DS | (0018,1111)
Distance Source to Support | DS | (0040,0307)
Distribution Address | LO | (4008,011A)
Distribution Name | PN | (4008,0119)
Doppler Correction Angle | FD | (0018,6034)
Doppler Sample Volume X Position | UL | (0018,6038)
Doppler Sample Volume Y Position | UL | (0018,603A)
Dose Calibration Factor | DS | (0054,1322)
Dose Comment | LO | (3004,0006)
Dose Grid Scaling | DS | (3004,000E)
Dose Rate Delivered | DS | (3008,0048)
Dose Rate Set | DS | (300A,0115)
Dose Reference Description | LO | (300A,0016)
Dose Reference Number | IS | (300A,0012)
Dose Reference Point Coordinates | DS | (300A,0018)
Dose Reference Sequence | SQ | (300A,0010)
Dose Reference Structure Type | CS | (300A,0014)
Dose Reference Type | CS | (300A,0020)
Dose Summation Type | CS | (3004,000A)
Dose Type | CS | (3004,0004)
Dose Units | CS | (3004,0002)
Dose Value | DS | (3004,0012)
DVH Data | DS | (3004,0058)
DVH Dose Scaling | DS | (3004,0052)
DVH Maximum Dose | DS | (3004,0072)
DVH Mean Dose | DS | (3004,0074)
DVH Minimum Dose | DS | (3004,0070)
DVH Normalization Dose Value | DS | (3004,0042)
DVH Normalization Point | DS | (3004,0040)
DVH Number of Bins | IS | (3004,0056)
DVH Referenced ROI Sequence | SQ | (3004,0060)
DVH ROI Contribution Type | CS | (3004,0062)
DVH Sequence | SQ | (3004,0050)
DVH Type | CS | (3004,0001)
DVH Volume Units | CS | (3004,0054)
Echo Number(s) | IS | (0018,0086)
Echo Time | DS | (0018,0081)
Echo Train Length | IS | (0018,0091)
Effective Series Duration | DS | (0018,0072)
Empty Image Density | CS | (2010,0110)
End Cumulative Meterset Weight | DS | (300C,0009)
End Meterset | DS | (3008,007A)
Energy Window Information Sequence | SQ | (0054,0012)
Energy Window Lower Limit | DS | (0054,0014)
Energy Window Name | SH | (0054,0018)
Energy Window Number | US | (0054,0308)
Energy Window Range Sequence | SQ | (0054,0013)
Energy Window Upper Limit | DS | (0054,0015)
Energy Window Vector | US | (0054,0010)
Entrance Dose | US | (0040,0302)
Entrance Dose in mGy | DS | (0040,8302)
Estimated Radiographic Magnification Factor | DS | (0018,1114)
Ethnic Group | SH | (0010,2160)
Event Elapsed Time(s) | DS | (0008,2130)
Event Timer Name(s) | LO | (0008,2132)
Execution Status | CS | (2100,0020)
Execution Status Info | CS | (2100,0030)
Expected Completion Date and Time | DT | (0040,4011)
Exposed Area | US | (0040,0303)
Exposure | IS | (0018,1152)
Exposure Control Mode | CS | (0018,7060)
Exposure Control Mode Description | LT | (0018,7062)
Exposure Dose Sequence | SQ | (0040,030E)
Exposure in uAs | IS | (0018,1153)
Exposure Sequence | SQ | (3002,0030)
Exposure Status | CS | (0018,7064)
Exposure Time | IS | (0018,1150)
Exposure Time in μS | DS | (0018,8150)
Exposures on Detector Since Last Calibration | IS | (0018,7010)
Exposures on Detector Since Manufactured | IS | (0018,7011)
Exposures on Plate | US | (0018,1404)
Failed SOP Instance UID List | UI | (0008,0058)
Failed SOP Sequence | SQ | (0008,1198)
Failure Reason | US | (0008,1197)
Field of View Dimension(s) | IS | (0018,1149)
Field of View Horizontal Flip | CS | (0018,7034)
Field of View Origin | DS | (0018,7030)
Field of View Rotation | DS | (0018,7032)
Field of View Shape | CS | (0018,1147)
File Meta Information Version | OB | (0002,0001)
File-set Consistency Flag | US | (0004,1212)
File-set Descriptor File ID | CS | (0004,1141)
File-set ID | CS | (0004,1130)
Filler Order Number / Imaging Service Request | LO | (0040,2017)
Film Box Content Sequence | SQ | (2130,0030)
Film Consumption Sequence | SQ | (0040,0321)
Film Destination | CS | (2000,0040)
Film Orientation | CS | (2010,0040)
Film Session Label | LO | (2000,0050)
Film Size ID | CS | (2010,0050)
Filter High Frequency | DS | (003A,0221)
Filter Low Frequency | DS | (003A,0220)
Filter Material | CS | (0018,7050)
Filter Thickness Maximum | DS | (0018,7054)
Filter Thickness Minimum | DS | (0018,7052)
Filter Type | SH | (0018,1160)
Final Cumulative Meterset Weight | DS | (300A,010E)
Final Cumulative Time Weight | DS | (300A,02C8)
First Treatment Date | DA | (3008,0054)
Fixation Device Description | ST | (300A,0196)
Fixation Device Label | SH | (300A,0194)
Fixation Device Position | SH | (300A,0198)
Fixation Device Sequence | SQ | (300A,0190)
Fixation Device Type | CS | (300A,0192)
Flip Angle | DS | (0018,1314)
Focal Distance | IS | (0018,1182)
Focal Spot(s) | DS | (0018,1190)
Focus Depth | DS | (0018,5012)
Fraction Group Number | IS | (300A,0071)
Fraction Group Sequence | SQ | (300A,0070)
Fraction Group Summary Sequence | SQ | (3008,0220)
Fraction Group Type | CS | (3008,0224)
Fraction Number | IS | (3002,0029)
Fraction Pattern | LT | (300A,007B)
Fraction Status Summary Sequence | SQ | (3008,0240)
Frame Delay | DS | (0018,1066)
Frame Increment Pointer | AT | (0028,0009)
Frame Label Vector | SH | (0018,2002)
Frame Numbers of Interest(FOI) | US | (0028,6020)
Frame of Reference Relationship Sequence | SQ | (3006,00C0)
Frame of Reference Transformation Comment | LO | (3006,00C8)
Frame of Reference Transformation Matrix | DS | (3006,00C6)
Frame of Reference Transformation Type | CS | (3006,00C4)
Frame of Reference UID | UI | (0020,0052)
Frame Primary Angle Vector | DS | (0018,2003)
Frame Reference Time | DS | (0054,1300)
Frame Secondary Angle Vector | DS | (0018,2004)
Frame Time | DS | (0018,1063)
Frame Time Vector | DS | (0018,1065)
Frame(s) of Interest Description | LO | (0028,6022)
Framing Type | LO | (0018,1064)
Gantry Angle | DS | (300A,011E)
Gantry Angle Tolerance | DS | (300A,0044)
Gantry Rotation Direction | CS | (300A,011F)
Gantry/Detector Slew | DS | (0018,1121)
Gantry/Detector Tilt | DS | (0018,1120)
Gated Information Sequence | SQ | (0054,0062)
General Purpose Performed Procedure Step Status | CS | (0040,4002)
General Purpose Scheduled Procedure Step Priority | CS | (0040,4003)
General Purpose Scheduled Procedure Step Status | CS | (0040,4001)
Generator Power | IS | (0018,1170)
Graphic Annotation Sequence | SQ | (0070,0001)
Graphic Annotation Units | CS | (0070,0005)
Graphic Data | FL | (0070,0022)
Graphic Dimensions | US | (0070,0020)
Graphic Filled | CS | (0070,0024)
Graphic Layer | CS | (0070,0002)
Graphic Layer Description | LO | (0070,0068)
Graphic Layer Order | IS | (0070,0062)
Graphic Layer Recommended Display Grayscale Value | US | (0070,0066)
Graphic Layer Recommended Display RGB Value | US | (0070,0067)
Graphic Layer Sequence | SQ | (0070,0060)
Graphic Object Sequence | SQ | (0070,0009)
Graphic Type | CS | (0070,0023)
Green Palette Color Lookup Table Data | OW | (0028,1202)
Green Palette Color Lookup Table Descriptor | US or SS | (0028,1102)
Grid | CS | (0018,1166)
Grid Absorbing Material | LT | (0018,7040)
Grid Aspect Ratio | IS | (0018,7046)
Grid Focal Distance | DS | (0018,704C)
Grid Frame Offset Vector | DS | (3004,000C)
Grid Period | DS | (0018,7048)
Grid Pitch | DS | (0018,7044)
Grid Spacing Material | LT | (0018,7041)
Grid Thickness | DS | (0018,7042)
Group Length | UL | (0002,0000)
Group Length | UL | (0004,0000)
Half Value Layer | DS | (0040,0314)
Hardcopy Creation Device ID | LO | (0018,1011)
Hardcopy Device Manufacturer’s Model Name | LO | (0018,101B)
Hardcopy Device Manufacturer | LO | (0018,1017)
Hardcopy Device Software Version | LO | (0018,101A)
Heart Rate | IS | (0018,1088)
High Bit | US | (0028,0102)
High R-R Value | IS | (0018,1082)
High-Dose Technique Type | CS | (300A,00C7)
Histogram Bin Width | US | (0060,3008)
Histogram Data | UL | (0060,3020)
Histogram Explanation | LO | (0060,3010)
Histogram First Bin Value | US or SS | (0060,3004)
Histogram Last Bin Value | US or SS | (0060,3006)
Histogram Number of Bins | US | (0060,3002)
Histogram Sequence | SQ | (0060,3000)
Human Performer Code Sequence | SQ | (0040,4009)
Human Performer's Name | PN | (0040,4037)
Human Performer's Organization | LO | (0040,4036)
Icon Image Sequence | SQ | (0088,0200)
Identical Documents Sequence | SQ | (0040,A525)
Illumination | US | (2010,015E)
Image Area Dose Product | DS | (0018,115E)
Image Box Content Sequence | SQ | (2130,0040)
Image Box Presentation LUT Flag | CS | (2000,006A)
Image Center Point Coordinates Sequence | SQ | (0040,071A)
Image Comments | LT | (0020,4000)
Image Display Format | ST | (2010,0010)
Image Frame Origin | US | (60xx,0051)
Image Horizontal Flip | CS | (0070,0041)
Image ID | SH | (0054,0400)
Image Index | US | (0054,1330)
Image Laterality | CS | (0020,0062)
Image Orientation (Patient) | DS | (0020,0037)
Image Overlay Box Content Sequence | SQ | (2130,0060)
Image Overlay Flag | CS | (2000,0067)
Image Plane Pixel Spacing | DS | (3002,0011)
Image Position | US | (2020,0010)
Image Position (Patient) | DS | (0020,0032)
Image Rotation | US | (0070,0042)
Image Transformation Matrix | DS | (0018,5210)
Image Translation Vector | DS | (0018,5212)
Image Trigger Delay | DS | (0018,1067)
Image Type | CS | (0008,0008)
Imaged Nucleus | SH | (0018,0085)
Imager Pixel Spacing | DS | (0018,1164)
Images in Acquisition | IS | (0020,1002)
Imaging Device-Specific Acquisition Parameters | LO | (300A,00CC)
Imaging Frequency | DS | (0018,0084)
Imaging Service Request Comments | LT | (0040,2400)
Implant Present | CS | (0028,1300)
Implementation Class UID | UI | (0002,0012)
Implementation Version Name | SH | (0002,0013)
Impressions | ST | (4008,0300)
Input Availability Flag | CS | (0040,4020)
Input Information Sequence | SQ | (0040,4021)
Instance Availability | CS | (0008,0056)
Instance Creation Date | DA | (0008,0012)
Instance Creation Time | TM | (0008,0013)
Instance Creator UID | UI | (0008,0014)
Instance Number | IS | (0020,0013)
Institution Address | ST | (0008,0081)
Institution Code Sequence | SQ | (0008,0082)
Institution Name | LO | (0008,0080)
Institutional Department Name | LO | (0008,1040)
Intensifier Size | DS | (0018,1162)
Inter-marker Distance | DS | (0050,0019)
Interpretation Approval Date | DA | (4008,0112)
Interpretation Approval Time | TM | (4008,0113)
Interpretation Approver Sequence | SQ | (4008,0111)
Interpretation Author | PN | (4008,010C)
Interpretation Diagnosis Code Sequence | SQ | (4008,0117)
Interpretation Diagnosis Description | LT | (4008,0115)
Interpretation ID | SH | (4008,0200)
Interpretation ID Issuer | LO | (4008,0202)
Interpretation Recorded Date | DA | (4008,0100)
Interpretation Recorded Time | TM | (4008,0101)
Interpretation Recorder | PN | (4008,0102)
Interpretation Status ID | CS | (4008,0212)
Interpretation Text | ST | (4008,010B)
Interpretation Transcriber | PN | (4008,010A)
Interpretation Transcription Date | DA | (4008,0108)
Interpretation Transcription Time | TM | (4008,0109)
Interpretation Type ID | CS | (4008,0210)
Intervals Acquired | IS | (0018,1083)
Intervals Rejected | IS | (0018,1084)
Intervention Drug Code Sequence | SQ | (0018,0029)
Intervention Drug Dose | DS | (0018,0028)
Intervention Drug Information Sequence | SQ | (0018,0026)
Intervention Drug Name | LO | (0018,0034)
Intervention Drug Start Time | TM | (0018,0035)
Intervention Drug Stop Time | TM | (0018,0027)
Interventional Status | CS | (0018,0038)
Interventional Therapy Sequence | SQ | (0018,0036)
Inversion Time | DS | (0018,0082)
Isocenter Position | DS | (300A,012C)
Issue Date of Imaging Service Request | DA | (0040,2004)
Issue Time of Imaging Service Request | TM | (0040,2005)
Issuer of Admission ID | LO | (0038,0011)
Issuer of Patient ID | LO | (0010,0021)
Item | Note: The VR for Item does not exist. See PS 3.5 for explanation. | (FFFE,E000)
Item Delimitation Item | Note: The VR for Item Delimitation Item does not exist. See PS 3.5 for explana-tion. | (FFFE,E00D)
Item Number | IS | (0020,0019)
IVUS Acquisition | CS | (0018,3100)
IVUS Gated Rate | DS | (0018,3102)
IVUS Pullback Rate | DS | (0018,3101)
IVUS Pullback Start Frame Number | IS | (0018,3103)
IVUS Pullback Stop Frame Number | IS | (0018,3104)
KVP | DS | (0018,0060)
Largest Image Pixel Value | US or SS | (0028,0107)
Largest Image Pixel Value in Plane | US or SS | (0028,0111)
Largest Pixel Value in Series | US or SS | (0028,0109)
Last Menstrual Date | DA | (0010,21D0)
Laterality | CS | (0020,0060)
Leaf Position Boundaries | DS | (300A,00BE)
Leaf/Jaw Positions | DS | (300A,011C)
Lesion Number | IS | (0018,3105)
Lookup Table (LUT) Number | IS | (0020,0026)
Lossy Image Compression | CS | (0028,2110)
Lossy Image Compression Ratio | DS | (0028,2112)
Low R-R Value | IS | (0018,1081)
LUT Data | US or SS or OW | (0028,3006)
LUT Descriptor | US or SS | (0028,3002)
LUT Explanation | LO | (0028,3003)
MAC Algorithm | CS | (0400,0015)
MAC Calculation Transfer Syntax UID | UI | (0400,0010)
MAC ID number | US | (0400,0005)
MAC Parameters Sequence | SQ | (4FFE,0001)
Magnetic Field Strength | DS | (0018,0087)
Magnification Type | CS | (2010,0060)
Magnify to Number of Columns | US | (2040,0074)
Manufacturer | LO | (0008,0070)
Manufacturer’s Model Name | LO | (0008,1090)
Mapping Resource | CS | (0008,0105)
Mask Frame Numbers | US | (0028,6110)
Mask Operation | CS | (0028,6101)
Mask Operation Explanation | ST | (0028,6190)
Mask Pointer(s) | US | (0028,6030)
Mask Sub-pixel Shift | FL | (0028,6114)
Mask Subtraction Sequence | SQ | (0028,6100)
Material ID | SH | (300A,00E1)
Max Density | US | (2010,0130)
Maximum Collated Films | IS | (2010,0154)
Maximum Coordinate Value | US | (50xx,0105)
Maximum Memory Allocation | IS | (2000,0061)
Measured Dose Description | ST | (3008,0012)
Measured Dose Reference Number | IS | (3008,0064)
Measured Dose Reference Sequence | SQ | (3008,0010)
Measured Dose Type | CS | (3008,0014)
Measured Dose Value | DS | (3008,0016)
Measured Value Sequence | SQ | (0040,A300)
Measurement Units Code Sequence | SQ | (0040,08EA)
Measuring Units Sequence | SQ | (0040,0295)
Mechanical Index | DS | (0018,5022)
Media Installed Sequence | SQ | (2000,00A2)
Media Storage SOP Class UID | UI | (0002,0002)
Media Storage SOP Instance UID | UI | (0002,0003)
Medical Alerts | LO | (0010,2000)
Medical Record Locator | LO | (0010,1090)
Medium Type | CS | (2000,0030)
Memory Allocation | IS | (2000,0060)
Memory Bit Depth | US | (2000,00A0)
Meterset Exposure | DS | (3002,0032)
Military Rank | LO | (0010,1080)
Min Density | US | (2010,0120)
Minimum Coordinate Value | US | (50xx,0104)
Modalities in Study | CS | (0008,0061)
Modality | CS | (0008,0060)
Modality LUT Sequence | SQ | (0028,3000)
Modality LUT Type | LO | (0028,3004)
Modifier Code Sequence | SQ | (0040,A195)
Most Recent Treatment Date | DA | (3008,0056)
MR Acquisition Type | CS | (0018,0023)
MRDR Directory Record Offset | UL | (0004,1504)
Multiple Copies Flag | CS | (0040,4006)
Multiplex Group Label | SH | (003A,0020)
Multiplex Group Time Offset | DS | (0018,1068)
Name of Physician(s) Reading Study | PN | (0008,1060)
Names of Intended Recipients of Results | PN | (0040,1010)
Nominal Beam Energy | DS | (300A,0114)
Nominal Beam Energy Unit | CS | (300A,0015)
Nominal Interval | IS | (0018,1062)
Nominal Prior Dose | DS | (300A,001A)
Nominal Scanned Pixel Spacing | DS | (0018,2010)
Non-DICOM Output Code Sequence | SQ | (0040,4032)
Normalization Point | DS | (3004,0008)
Notch Filter Bandwidth | DS | (003A,0223)
Notch Filter Frequency | DS | (003A,0222)
Number of Averages | DS | (0018,0083)
Number of Beams | IS | (300A,0080)
Number of Blocks | IS | (300A,00F0)
Number of Boli | IS | (300A,00ED)
Number of Brachy Application Setups | IS | (300A,00A0)
Number of Channels | US | (50xx,2004)
Number of Compensators | IS | (300A,00E0)
Number of Contour Points | IS | (3006,0046)
Number of Control Points | IS | (300A,0110)
Number of Copies | IS | (2000,0010)
Number of Detectors | US | (0054,0021)
Number of Energy Windows | US | (0054,0011)
Number of Event Timers | IS | (0008,2129)
Number of Films | IS | (2100,0170)
Number of Fraction Pattern Digits Per Day | IS | (300A,0079)
Number of Fractions Delivered | IS | (3008,005A)
Number of Fractions Planned | IS | (300A,0078)
Number of Frames | IS | (0028,0008)
Number of Frames in Overlay | IS | (60xx,0015)
Number of Frames in Phase | US | (0054,0033)
Number of Frames in Rotation | US | (0054,0053)
Number of Graphic Points | US | (0070,0021)
Number of Leaf/Jaw Pairs | IS | (300A,00BC)
Number of Patient Related Instances | IS | (0020,1204)
Number of Patient Related Series | IS | (0020,1202)
Number of Patient Related Studies | IS | (0020,1200)
Number of Phase Encoding Steps | IS | (0018,0089)
Number of Phases | US | (0054,0031)
Number of Points | US | (50xx,0010)
Number of Pulses | IS | (300A,028A)
Number of References | UL | (0004,1600)
Number of Rotations | US | (0054,0051)
Number of R-R Intervals | US | (0054,0061)
Number of Samples | UL | (50xx,2006)
Number of Series Related Instances | IS | (0020,1209)
Number of Slices | US | (0054,0081)
Number of Stages | IS | (0008,2124)
Number of Study Related Instances | IS | (0020,1208)
Number of Study Related Series | IS | (0020,1206)
Number of Table Break Points | UL | (0018,6050)
Number of Table Entries | UL | (0018,6056)
Number of Temporal Positions | IS | (0020,0105)
Number of Time Slices | US | (0054,0101)
Number of Time Slots | US | (0054,0071)
Number of Tomosynthesis Source Images | IS | (0018,1495)
Number of Triggers in Phase | US | (0054,0211)
Number of Views in Stage | IS | (0008,212A)
Number of Waveform Channels | US | (003A,0005)
Number of Waveform Samples | UL | (003A,0010)
Number of Wedges | IS | (300A,00D0)
Numeric Value | DS | (0040,A30A)
Observation DateTime | DT | (0040,A032)
Observation Number | IS | (3006,0082)
Occupation | SH | (0010,2180)
Offset of Referenced Lower-Level Directory Entity | UL | (0004,1420)
Offset of the First Directory Record of the Root Directory Entity | UL | (0004,1200)
Offset of the Last Directory Record of the Root Directory Entity | UL | (0004,1202)
Offset of the Next Directory Record | UL | (0004,1400)
Operators’ Name | PN | (0008,1070)
Order Callback Phone Number | SH | (0040,2010)
Order Entered By | PN | (0040,2008)
Order Enterer’s Location | SH | (0040,2009)
Organ at Risk Full-volume Dose | DS | (300A,002A)
Organ at Risk Limit Dose | DS | (300A,002B)
Organ at Risk Maximum Dose | DS | (300A,002C)
Organ at Risk Overdose Volume Fraction | DS | (300A,002D)
Organ Dose | DS | (0040,0316)
Organ Exposed | CS | (0040,0318)
Original Image Sequence | SQ | (2130,00C0)
Originator | AE | (2100,0070)
Other Magnification Types Available | CS | (2010,00A7)
Other Media Available Sequence | SQ | (2000,00A4)
Other Patient IDs | LO | (0010,1000)
Other Patient Names | PN | (0010,1001)
Other Smoothing Types Available | CS | (2010,00A9)
Other Study Numbers | IS | (0020,1070)
Output Information Sequence | SQ | (0040,4033)
Output Power | SH | (0018,5000)
Overlay Activation Layer | CS | (60xx,1001)
Overlay Background Density | CS | (2040,0082)
Overlay Bit Position | US | (60xx,0102)
Overlay Bits Allocated | US | (60xx,0100)
Overlay Columns | US | (60xx,0011)
Overlay Data | OB or OW | (60xx,3000)
Overlay Date | DA | (0008,0024)
Overlay Description | LO | (60xx,0022)
Overlay Foreground Density | CS | (2040,0080)
Overlay Label | LO | (60xx,1500)
Overlay Magnification Type | CS | (2040,0060)
Overlay Number | IS | (0020,0022)
Overlay or Image Magnification | CS | (2040,0072)
Overlay Origin | SS | (60xx,0050)
Overlay Pixel Data Sequence | SQ | (2040,0020)
Overlay Plane Origin | US | (60xx,0052)
Overlay Planes | US | (60xx,0012)
Overlay Rows | US | (60xx,0010)
Overlay Smoothing Type | CS | (2040,0070)
Overlay Subtype | LO | (60xx,0045)
Overlay Time | TM | (0008,0034)
Overlay Type | CS | (60xx,0040)
Override Parameter Pointer | AT | (3008,0062)
Override Reason | ST | (3008,0066)
Override Sequence | SQ | (3008,0060)
Owner ID | SH | (2100,0160)
Page Number Vector | IS | (0018,2001)
Palette Color Lookup Table UID | UI | (0028,1199)
Partial View | CS | (0028,1350)
Partial View Description | ST | (0028,1351)
Patient Additional Position | LO | (300A,0184)
Patient Comments | LT | (0010,4000)
Patient Gantry Relationship Code Sequence | SQ | (0054,0414)
Patient ID | LO | (0010,0020)
Patient Orientation | CS | (0020,0020)
Patient Orientation Code Sequence | SQ | (0054,0410)
Patient Orientation Modifier Code Sequence | SQ | (0054,0412)
Patient Position | CS | (0018,5100)
Patient Setup Number | IS | (300A,0182)
Patient Setup Sequence | SQ | (300A,0180)
Patient State | LO | (0038,0500)
Patient Support Angle | DS | (300A,0122)
Patient Support Angle Tolerance | DS | (300A,004C)
Patient Support Rotation Direction | CS | (300A,0123)
Patient Transport Arrangements | LO | (0040,1004)
Patient’s Name | PN | (0010,0010)
Patient’s Primary Language Code Modifier Sequence | SQ | (0010,0102)
Patient’s Primary Language Code Sequence | SQ | (0010,0101)
Patient’s Telephone Numbers | SH | (0010,2154)
Patient's Address | LO | (0010,1040)
Patient's Age | AS | (0010,1010)
Patient's Birth Date | DA | (0010,0030)
Patient's Birth Name | PN | (0010,1005)
Patient's Birth Time | TM | (0010,0032)
Patient's Institution Residence | LO | (0038,0400)
Patient's Insurance Plan Code Sequence | SQ | (0010,0050)
Patient's Mother's Birth Name | PN | (0010,1060)
Patient's Religious Preference | LO | (0010,21F0)
Patient's Sex | CS | (0010,0040)
Patient's Size | DS | (0010,1020)
Patient's Weight | DS | (0010,1030)
Pause Between Frames | IS | (0054,0038)
Percent Phase Field of View | DS | (0018,0094)
Percent Sampling | DS | (0018,0093)
Performed Location | SH | (0040,0243)
Performed Procedure Code Sequence | SQ | (0040,A372)
Performed Procedure Step Description | LO | (0040,0254)
Performed Procedure Step End Date | DA | (0040,0250)
Performed Procedure Step End Time | TM | (0040,0251)
Performed Procedure Step ID | SH | (0040,0253)
Performed Procedure Step Start Date | DA | (0040,0244)
Performed Procedure Step Start Time | TM | (0040,0245)
Performed Procedure Step Status | CS | (0040,0252)
Performed Procedure Type Description | LO | (0040,0255)
Performed Processing Applications Code Sequence | SQ | (0040,4007)
Performed Protocol Code Sequence | SQ | (0040,0260)
Performed Series Sequence | SQ | (0040,0340)
Performed Station AE Title | AE | (0040,0241)
Performed Station Class Code Sequence | SQ | (0040,4029)
Performed Station Geographic Location Code Sequence | SQ | (0040,4030)
Performed Station Name | SH | (0040,0242)
Performed Station Name Code Sequence | SQ | (0040,4028)
Performed Workitem Code Sequence | SQ | (0040,4019)
Performing Physician’s Name | PN | (0008,1050)
Person Name | PN | (0040,A123)
Pertinent Other Evidence Sequence | SQ | (0040,A385)
Phase Delay | IS | (0054,0036)
Phase Encoding Direction | CS | (0018,1312)
Phase Information Sequence | SQ | (0054,0032)
Phase Vector | US | (0054,0030)
Phosphor Type | LO | (0018,1261)
Photometric Interpretation | CS | (0028,0004)
Phototimer Setting | DS | (0018,7065)
Physical Delta X | FD | (0018,602C)
Physical Delta Y | FD | (0018,602E)
Physical Units X Direction | US | (0018,6024)
Physical Units Y Direction | US | (0018,6026)
Physician Approving Interpretation | PN | (4008,0114)
Physician(s) of Record | PN | (0008,1048)
Pixel Aspect Ratio | IS | (0028,0034)
Pixel Bandwidth | DS | (0018,0095)
Pixel Component Data Type | US | (0018,604E)
Pixel Component Mask | UL | (0018,6046)
Pixel Component Organization | US | (0018,6044)
Pixel Component Physical Units | US | (0018,604C)
Pixel Component Range Start | UL | (0018,6048)
Pixel Component Range Stop | UL | (0018,604A)
Pixel Data | OW or OB | (7FE0,0010)
Pixel Intensity Relationship | CS | (0028,1040)
Pixel Intensity Relationship Sign | SS | (0028,1041)
Pixel Padding Value | US or SS | (0028,0120)
Pixel Representation | US | (0028,0103)
Pixel Spacing | DS | (0028,0030)
Pixel Spacing Sequence | SQ | (0040,08D8)
Placer Order Number / Imaging Service Request | LO | (0040,2016)
Planar Configuration | US | (0028,0006)
Planes | US | (0028,0012)
Planned Verification Image Sequence | SQ | (300A,00CA)
Plate ID | LO | (0018,1004)
Plate Type | SH | (0018,1260)
Polarity | CS | (2020,0020)
Position Reference Indicator | LO | (0020,1040)
Positioner Motion | CS | (0018,1500)
Positioner Primary Angle | DS | (0018,1510)
Positioner Primary Angle Increment | DS | (0018,1520)
Positioner Secondary Angle | DS | (0018,1511)
Positioner Secondary Angle Increment | DS | (0018,1521)
Positioner Type | CS | (0018,1508)
Postprocessing Function | LO | (0018,5021)
Predecessor Documents Sequence | SQ | (0040,A360)
Preferred Playback Sequencing | US | (0018,1244)
Pregnancy Status | US | (0010,21C0)
Pre-Medication | LO | (0040,0012)
Prescription Description | ST | (300A,000E)
Presentation Creation Date | DA | (0070,0082)
Presentation Creation Time | TM | (0070,0083)
Presentation Creator’s Name | PN | (0070,0084)
Presentation Description | LO | (0070,0081)
Presentation Intent Type | CS | (0008,0068)
Presentation Label | CS | (0070,0080)
Presentation LUT Content Sequence | SQ | (2130,0080)
Presentation LUT Flag | CS | (2000,0069)
Presentation LUT Sequence | SQ | (2050,0010)
Presentation LUT Shape | CS | (2050,0020)
Presentation Pixel Aspect Ratio | IS | (0070,0102)
Presentation Pixel Magnification Ratio | FL | (0070,0103)
Presentation Pixel Spacing | DS | (0070,0101)
Presentation Size Mode | CS | (0070,0100)
Primary Anatomic Structure Modifier Sequence | SQ | (0008,2230)
Primary Anatomic Structure Sequence | SQ | (0008,2228)
Primary Dosimeter Unit | CS | (300A,00B3)
Primary(Prompts) Counts Accumulated | IS | (0054,1310)
Print Job Description Sequence | SQ | (2120,0050)
Print Job ID | SH | (2100,0010)
Print Management Capabilities Sequence | SQ | (2130,0010)
Print Priority | CS | (2000,0020)
Print Queue ID | SH | (2110,0099)
Printer Characteristics Sequence | SQ | (2130,0015)
Printer Configuration Sequence | SQ | (2000,001E)
Printer Name | LO | (2110,0030)
Printer Pixel Spacing | DS | (2010,0376)
Printer Resolution ID | CS | (2010,0052)
Printer Status | CS | (2110,0010)
Printer Status Info | CS | (2110,0020)
Printing Bit Depth | US | (2000,00A1)
Private Coding Scheme Creator UID | UI | (0008,010C)
Private Information | OB | (0002,0102)
Private Information Creator UID | UI | (0002,0100)
Private Record UID | UI | (0004,1432)
Procedure Code Sequence | SQ | (0008,1032)
Processing Function | LO | (0018,5020)
Projection Eponymous Name Code Sequence | SQ | (0018,5104)
Proposed Study Sequence | SQ | (2130,00A0)
Protocol Name | LO | (0018,1030)
Pulse Repetition Frequency | UL | (0018,6032)
Pulse Repetition Interval | DS | (300A,028C)
Purpose of Reference Code Sequence | SQ | (0040,A170)
PVC Rejection | LO | (0018,1085)
Quality Control Image | CS | (0028,0300)
Quantity | DS | (0040,0294)
Quantity Sequence | SQ | (0040,0293)
Query/Retrieve Level | CS | (0008,0052)
Queue Status | CS | (2120,0010)
R Wave Pointer | US | (0028,6040)
Radial Position | DS | (0018,1142)
Radiation Machine Name | SH | (3002,0020)
Radiation Machine SAD | DS | (3002,0022)
Radiation Machine SSD | DS | (3002,0024)
Radiation Mode | CS | (0018,115A)
Radiation Setting | CS | (0018,1155)
Radiation Type | CS | (300A,00C6)
Radionuclide Code Sequence | SQ | (0054,0300)
Radionuclide Half Life | DS | (0018,1075)
Radionuclide Positron Fraction | DS | (0018,1076)
Radionuclide Total Dose | DS | (0018,1074)
Radiopharmaceutical | LO | (0018,0031)
Radiopharmaceutical Code Sequence | SQ | (0054,0304)
Radiopharmaceutical Information Sequence | SQ | (0054,0016)
Radiopharmaceutical Route | LO | (0018,1070)
Radiopharmaceutical Specific Activity | DS | (0018,1077)
Radiopharmaceutical Start Time | TM | (0018,1072)
Radiopharmaceutical Stop Time | TM | (0018,1073)
Radiopharmaceutical Volume | DS | (0018,1071)
Radius of Circular Collimator | IS | (0018,1712)
Radius of Circular Shutter | IS | (0018,1612)
Randoms Correction Method | CS | (0054,1100)
Reason for Study | LO | (0032,1030)
Reason for the Imaging Service Request | LO | (0040,2001)
Reason for the Requested Procedure | LO | (0040,1002)
Receiving Coil | SH | (0018,1250)
Recommended Display Frame Rate | IS | (0008,2144)
Recommended Viewing Mode | CS | (0028,1090)
Reconstruction Diameter | DS | (0018,1100)
Reconstruction Method | LO | (0054,1103)
Record In-use Flag | US | (0004,1410)
Recorded Block Sequence | SQ | (3008,00D0)
Recorded Brachy Accessory Device Sequence | SQ | (3008,0120)
Recorded Channel Sequence | SQ | (3008,0130)
Recorded Channel Shield Sequence | SQ | (3008,0150)
Recorded Compensator Sequence | SQ | (3008,00C0)
Recorded Source Applicator Sequence | SQ | (3008,0140)
Recorded Source Sequence | SQ | (3008,0100)
Recorded Wedge Sequence | SQ | (3008,00B0)
Rectification Type | CS | (0018,1156)
Red Palette Color Lookup Table Data | OW | (0028,1201)
Red Palette Color Lookup Table Descriptor | US or SS | (0028,1101)
Reference Air Kerma Rate | DS | (300A,022A)
Reference Image Number | IS | (300A,00C8)
Reference Pixel Physical Value X | FD | (0018,6028)
Reference Pixel Physical Value Y | FD | (0018,602A)
Reference Pixel X0 | SL | (0018,6020)
Reference Pixel Y0 | SL | (0018,6022)
Reference to Recorded Sound | LO | (4008,0103)
Referenced Basic Annotation Box Sequence | SQ | (2010,0520)
Referenced Beam Number | IS | (300C,0006)
Referenced Beam Sequence | SQ | (300C,0004)
Referenced Block Number | IS | (300C,00E0)
Referenced Bolus Sequence | SQ | (300C,00B0)
Referenced Brachy Accessory Device Number | IS | (3008,0122)
Referenced Brachy Application Setup Number | IS | (300C,000C)
Referenced Brachy Application Setup Sequence | SQ | (300C,000A)
Referenced Calculated Dose Reference Number | IS | (3008,0092)
Referenced Calculated Dose Reference Sequence | SQ | (3008,0090)
Referenced Channel Shield Number | IS | (3008,0152)
Referenced Compensator Number | IS | (300C,00D0)
Referenced Content Item Identifier | UL | (0040,DB73)
Referenced Control Point Index | IS | (300C,00F0)
Referenced Curve Sequence | SQ | (0008,1145)
Referenced Datetime | DT | (0040,A13A)
Referenced Dose Reference Number | IS | (300C,0051)
Referenced Dose Reference Sequence | SQ | (300C,0050)
Referenced Dose Sequence | SQ | (300C,0080)
Referenced File ID | CS | (0004,1500)
Referenced Film Box Sequence | SQ | (2000,0500)
Referenced Film Session Sequence | SQ | (2010,0500)
Referenced Fraction Group Number | IS | (300C,0022)
Referenced Fraction Group Sequence | SQ | (300C,0020)
Referenced Fraction Number | IS | (3008,0223)
Referenced Frame Number | IS | (0008,1160)
Referenced Frame Numbers | US | (0040,A136)
Referenced Frame of Reference Sequence | SQ | (3006,0010)
Referenced Frame of Reference UID | UI | (3006,0024)
Referenced General Purpose Scheduled Procedure Step Sequence | SQ | (0040,4016)
Referenced General Purpose Scheduled Procedure Step Transaction UID | UI | (0040,4023)
Referenced Image Box Sequence | SQ | (2010,0510)
Referenced Image Sequence | SQ | (0008,1140)
Referenced Instance Sequence | SQ | (0008,114A)
Referenced Interpretation Sequence | SQ | (4008,0050)
Referenced Measured Dose Reference Number | IS | (3008,0082)
Referenced Measured Dose Reference Sequence | SQ | (3008,0080)
Referenced Non-Image Composite SOP Instance Sequence | SQ | (0040,0220)
Referenced Overlay Group | US | (50xx,2610)
Referenced Overlay Plane Groups | US | (2040,0011)
Referenced Overlay Plane Sequence | SQ | (2040,0010)
Referenced Overlay Sequence | SQ | (0008,1130)
Referenced Overlay Sequence | SQ | (50xx,2600)
Referenced Patient Alias Sequence | SQ | (0038,0004)
Referenced Patient Sequence | SQ | (0008,1120)
Referenced Patient Setup Number | IS | (300C,006A)
Referenced Presentation LUT Sequence | SQ | (2050,0500)
Referenced Print Job Sequence | SQ | (2100,0500)
Referenced Print Job Sequence | SQ | (2120,0070)
Referenced Procedure Step Sequence | SQ | (0040,0330)
Referenced Reference Image Number | IS | (300C,0007)
Referenced Reference Image Sequence | SQ | (300C,0042)
Referenced Request Sequence | SQ | (0040,A370)
Referenced Results Sequence | SQ | (0008,1100)
Referenced ROI Number | IS | (3006,0084)
Referenced RT Plan Sequence | SQ | (300C,0002)
Referenced Sample Positions | UL | (0040,A132)
Referenced Series Sequence | SQ | (0008,1115)
Referenced SOP Class UID | UI | (0008,1150)
Referenced SOP Class UID in File | UI | (0004,1510)
Referenced SOP Instance UID | UI | (0008,1155)
Referenced SOP Instance UID in File | UI | (0004,1511)
Referenced SOP Sequence | SQ | (0008,1199)
Referenced Source Applicator Number | IS | (3008,0142)
Referenced Source Number | IS | (300C,000E)
Referenced Stored Print Sequence | SQ | (2000,0510)
Referenced Structure Set Sequence | SQ | (300C,0060)
Referenced Study Component Sequence | SQ | (0008,1111)
Referenced Study Sequence | SQ | (0008,1110)
Referenced Time Offsets | DS | (0040,A138)
Referenced Tolerance Table Number | IS | (300C,00A0)
Referenced Transfer Syntax UID in File | UI | (0004,1512)
Referenced Treatment Record Sequence | SQ | (3008,0030)
Referenced Verification Image Sequence | SQ | (300C,0040)
Referenced Visit Sequence | SQ | (0008,1125)
Referenced Waveform Channels | US | (0040,A0B0)
Referenced Waveform Sequence | SQ | (0008,113A)
Referenced Wedge Number | IS | (300C,00C0)
Referring Physician’s Name | PN | (0008,0090)
Referring Physician’s Telephone Numbers | SH | (0008,0094)
Referring Physician's Address | ST | (0008,0092)
Reflected Ambient Light | US | (2010,0160)
Region Data Type | US | (0018,6014)
Region Flags | UL | (0018,6016)
Region Location Max X1 | UL | (0018,601C)
Region Location Max Y1 | UL | (0018,601E)
Region Location Min X0 | UL | (0018,6018)
Region Location Min Y0 | UL | (0018,601A)
Region of Residence | LO | (0010,2152)
Region Spatial Format | US | (0018,6012)
Related Frame of Reference UID | UI | (3006,00C2)
Related RT ROI Observations Sequence | SQ | (3006,00A0)
Relationship Type | CS | (0040,A010)
Relative X-ray Exposure | IS | (0018,1405)
Relevant Information Sequence | SQ | (0040,4022)
Repeat Fraction Cycle Length | IS | (300A,007A)
Repetition Time | DS | (0018,0080)
Reported Values Origin | CS | (3002,000A)
Reporting Priority | SH | (0040,1009)
Representative Frame Number | US | (0028,6010)
Reprojection Method | CS | (0054,1004)
Request Attributes Sequence | SQ | (0040,0275)
Requested Contrast Agent | LO | (0032,1070)
Requested Decimate/Crop Behavior | CS | (2020,0040)
Requested Image Size | DS | (2020,0030)
Requested Image Size Flag | CS | (2020,00A0)
Requested Procedure Code Sequence | SQ | (0032,1064)
Requested Procedure Comments | LT | (0040,1400)
Requested Procedure Description | LO | (0032,1060)
Requested Procedure ID | SH | (0040,1001)
Requested Procedure Location | LO | (0040,1005)
Requested Procedure Priority | SH | (0040,1003)
Requested Resolution ID | CS | (2020,0050)
Requested Subsequent Workitem Code Sequence | SQ | (0040,4031)
Requesting Physician | PN | (0032,1032)
Requesting Service | LO | (0032,1033)
Rescale Intercept | DS | (0028,1052)
Rescale Slope | DS | (0028,1053)
Rescale Type | LO | (0028,1054)
Residual Syringe Counts | IS | (0054,0017)
Resulting General Purpose Performed Procedure Steps Sequence | SQ | (0040,4015)
Results Comments | ST | (4008,4000)
Results Distribution List Sequence | SQ | (4008,0118)
Results ID | SH | (4008,0040)
Results ID Issuer | LO | (4008,0042)
Retrieve AE Title | AE | (0008,0054)
Review Date | DA | (300E,0004)
Review Time | TM | (300E,0005)
Reviewer Name | PN | (300E,0008)
ROI Area | IS | (60xx,1301)
ROI Contour Sequence | SQ | (3006,0039)
ROI Description | ST | (3006,0028)
ROI Display Color | IS | (3006,002A)
ROI Generation Algorithm | CS | (3006,0036)
ROI Generation Description | LO | (3006,0038)
ROI Interpreter | PN | (3006,00A6)
ROI Mean | DS | (60xx,1302)
ROI Name | LO | (3006,0026)
ROI Number | IS | (3006,0022)
ROI Observation Description | ST | (3006,0088)
ROI Observation Label | SH | (3006,0085)
ROI Physical Properties Sequence | SQ | (3006,00B0)
ROI Physical Property | CS | (3006,00B2)
ROI Physical Property Value | DS | (3006,00B4)
ROI Standard Deviation | DS | (60xx,1303)
ROI Volume | DS | (3006,002C)
Rotation Direction | CS | (0018,1140)
Rotation Information Sequence | SQ | (0054,0052)
Rotation of Scanned Film | DS | (0018,2030)
Rotation Vector | US | (0054,0050)
Route of Admissions | LO | (0038,0016)
Rows | US | (0028,0010)
R-R Interval Vector | US | (0054,0060)
RT Beam Limiting Device Type | CS | (300A,00B8)
RT Dose ROI Sequence | SQ | (3004,0010)
RT Image Description | ST | (3002,0004)
RT Image Label | SH | (3002,0002)
RT Image Name | LO | (3002,0003)
RT Image Orientation | DS | (3002,0010)
RT Image Plane | CS | (3002,000C)
RT Image Position | DS | (3002,0012)
RT Image SID | DS | (3002,0026)
RT Plan Date | DA | (300A,0006)
RT Plan Description | ST | (300A,0004)
RT Plan Geometry | CS | (300A,000C)
RT Plan Label | SH | (300A,0002)
RT Plan Name | LO | (300A,0003)
RT Plan Relationship | CS | (300A,0055)
RT Plan Time | TM | (300A,0007)
RT Referenced Series Sequence | SQ | (3006,0014)
RT Referenced Study Sequence | SQ | (3006,0012)
RT Related ROI Sequence | SQ | (3006,0030)
RT ROI Identification Code Sequence | SQ | (3006,0086)
RT ROI Interpreted Type | CS | (3006,00A4)
RT ROI Observations Sequence | SQ | (3006,0080)
RT ROI Relationship | CS | (3006,0033)
Safe Position Exit Date | DA | (3008,0162)
Safe Position Exit Time | TM | (3008,0164)
Safe Position Return Date | DA | (3008,0166)
Safe Position Return Time | TM | (3008,0168)
Sample Rate | UL | (50xx,2008)
Samples per Pixel | US | (0028,0002)
Sampling Frequency | DS | (003A,001A)
SAR | DS | (0018,1316)
Scan Arc | DS | (0018,1143)
Scan Length | IS | (0018,1302)
Scan Options | CS | (0018,0022)
Scan Velocity | DS | (0018,1300)
Scanning Sequence | CS | (0018,0020)
Scatter Correction Method | LO | (0054,1105)
Scatter Fraction Factor | DS | (0054,1323)
Scheduled Admission Date | DA | (0038,001A)
Scheduled Admission Time | TM | (0038,001B)
Scheduled Discharge Date | DA | (0038,001C)
Scheduled Discharge Time | TM | (0038,001D)
Scheduled Human Performers Sequence | SQ | (0040,4034)
Scheduled Patient Institution Residence | LO | (0038,001E)
Scheduled Performing Physician's Name | PN | (0040,0006)
Scheduled Procedure Step Description | LO | (0040,0007)
Scheduled Procedure Step End Date | DA | (0040,0004)
Scheduled Procedure Step End Time | TM | (0040,0005)
Scheduled Procedure Step ID | SH | (0040,0009)
Scheduled Procedure Step Location | SH | (0040,0011)
Scheduled Procedure Step Sequence | SQ | (0040,0100)
Scheduled Procedure Step Start Date | DA | (0040,0002)
Scheduled Procedure Step Start Date and Time | DT | (0040,4005)
Scheduled Procedure Step Start Time | TM | (0040,0003)
Scheduled Procedure Step Status | CS | (0040,0020)
Scheduled Processing Applications Code Sequence | SQ | (0040,4004)
Scheduled Protocol Code Sequence | SQ | (0040,0008)
Scheduled Station AE Title | AE | (0040,0001)
Scheduled Station Class Code Sequence | SQ | (0040,4026)
Scheduled Station Geographic Location Code Sequence | SQ | (0040,4027)
Scheduled Station Name | SH | (0040,0010)
Scheduled Station Name Code Sequence | SQ | (0040,4025)
Scheduled Step Attributes Sequence | SQ | (0040,0270)
Scheduled Study Location | LO | (0032,1020)
Scheduled Study Location AE Title(s) | AE | (0032,1021)
Scheduled Study Start Date | DA | (0032,1000)
Scheduled Study Start Time | TM | (0032,1001)
Scheduled Study Stop Date | DA | (0032,1010)
Scheduled Study Stop Time | TM | (0032,1011)
Scheduled Workitem Code Sequence | SQ | (0040,4018)
Secondary Capture Device ID | LO | (0018,1010)
Secondary Capture Device Manufacturer | LO | (0018,1016)
Secondary Capture Device Manufacturer’s Model Name | LO | (0018,1018)
Secondary Capture Device Software Version(s) | LO | (0018,1019)
Secondary Counts Accumulated | IS | (0054,1311)
Secondary Counts Type | CS | (0054,1220)
Segmented Blue Palette Color Lookup Table Data | OW | (0028,1223)
Segmented Green Palette Color Lookup Table Data | OW | (0028,1222)
Segmented Red Palette Color Lookup Table Data | OW | (0028,1221)
Sensitivity | DS | (0018,6000)
Sequence Delimitation Item | Note: The VR for Sequence Delimitation Item does not exist. See PS 3.5 for explanation. | (FFFE,E0DD)
Sequence Name | SH | (0018,0024)
Sequence of Ultrasound Regions | SQ | (0018,6011)
Sequence Variant | CS | (0018,0021)
Series Date | DA | (0008,0021)
Series Description | LO | (0008,103E)
Series in Study | IS | (0020,1000)
Series Instance UID | UI | (0020,000E)
Series Number | IS | (0020,0011)
Series Time | TM | (0008,0031)
Series Type | CS | (0054,1000)
Setup Device Description | ST | (300A,01BA)
Setup Device Label | SH | (300A,01B8)
Setup Device Parameter | DS | (300A,01BC)
Setup Device Sequence | SQ | (300A,01B4)
Setup Device Type | CS | (300A,01B6)
Setup Reference Description | ST | (300A,01D0)
Setup Technique | CS | (300A,01B0)
Setup Technique Description | ST | (300A,01B2)
Shielding Device Description | ST | (300A,01A6)
Shielding Device Label | SH | (300A,01A4)
Shielding Device Position | SH | (300A,01A8)
Shielding Device Sequence | SQ | (300A,01A0)
Shielding Device Type | CS | (300A,01A2)
Shutter Left Vertical Edge | IS | (0018,1602)
Shutter Lower Horizontal Edge | IS | (0018,1608)
Shutter Overlay Group | US | (0018,1623)
Shutter Presentation Value | US | (0018,1622)
Shutter Right Vertical Edge | IS | (0018,1604)
Shutter Shape | CS | (0018,1600)
Shutter Upper Horizontal Edge | IS | (0018,1606)
Signature | OB | (0400,0120)
Skip Beats | IS | (0018,1086)
Slice Location | DS | (0020,1041)
Slice Location Vector | DS | (0018,2005)
Slice Sensitivity Factor | DS | (0054,1320)
Slice Thickness | DS | (0018,0050)
Slice Vector | US | (0054,0080)
Slide Identifier | LO | (0040,06FA)
Smallest Image Pixel Value | US or SS | (0028,0106)
Smallest Image Pixel Value in Plane | US or SS | (0028,0110)
Smallest Pixel Value in Series | US or SS | (0028,0108)
Smoking Status | CS | (0010,21A0)
Smoothing Type | CS | (2010,0080)
Soft Tissue Thermal Index | DS | (0018,5027)
Soft Tissue-focus Thermal Index | DS | (0018,5028)
Soft Tissue-surface Thermal Index | DS | (0018,5029)
Softcopy VOI LUT Sequence | SQ | (0028,3110)
Software Version(s) | LO | (0018,1020)
SOP Authorization Comment | LT | (0100,0424)
SOP Authorization Date and Time | DT | (0100,0420)
SOP Class UID | UI | (0008,0016)
SOP Classes Supported | UI | (0008,115A)
SOP Instance Status | CS | (0100,0410)
SOP Instance UID | UI | (0008,0018)
Source Application Entity Title | AE | (0002,0016)
Source Applicator ID | SH | (300A,0291)
Source Applicator Length | DS | (300A,0296)
Source Applicator Manufacturer | LO | (300A,0298)
Source Applicator Name | LO | (300A,0294)
Source Applicator Number | IS | (300A,0290)
Source Applicator Step Size | DS | (300A,02A0)
Source Applicator Type | CS | (300A,0292)
Source Applicator Wall Nominal Thickness | DS | (300A,029C)
Source Applicator Wall Nominal Transmission | DS | (300A,029E)
Source Encapsulation Nominal Thickness | DS | (300A,0222)
Source Encapsulation Nominal Transmission | DS | (300A,0224)
Source Image Sequence | SQ | (0008,2112)
Source Isotope Half Life | DS | (300A,0228)
Source Isotope Name | LO | (300A,0226)
Source Manufacturer | LO | (300A,0216)
Source Movement Type | CS | (300A,0288)
Source Number | IS | (300A,0212)
Source Sequence | SQ | (300A,0210)
Source Serial Number | LO | (3008,0105)
Source to Beam Limiting Device Distance | DS | (300A,00BA)
Source to Block Tray Distance | DS | (300A,00F6)
Source to Compensator Tray Distance | DS | (300A,00E6)
Source to Reference Object Distance | DS | (3002,0028)
Source to Surface Distance | DS | (300A,0130)
Source to Wedge Tray Distance | DS | (300A,00DA)
Source Type | CS | (300A,0214)
Source Waveform Sequence | SQ | (003A,020A)
Source-Axis Distance | DS | (300A,00B4)
Spacing Between Slices | DS | (0018,0088)
Spatial Resolution | DS | (0018,1050)
Special Needs | LO | (0038,0050)
Specific Character Set | CS | (0008,0005)
Specific Character Set of File-set Descriptor File | CS | (0004,1142)
Specified Channel Total Time | DS | (3008,0132)
Specified Meterset | DS | (3008,0042)
Specified Number of Pulses | IS | (3008,0136)
Specified Primary Meterset | DS | (3008,0032)
Specified Pulse Repetition Interval | DS | (3008,013A)
Specified Secondary Meterset | DS | (3008,0033)
Specified Treatment Time | DS | (3008,003A)
Specimen Accession Number | LO | (0040,050A)
Specimen Identifier | LO | (0040,0551)
Specimen Sequence | SQ | (0040,0550)
Specimen Type Code Sequence | SQ | (0040,059A)
Stage Code Sequence | SQ | (0040,000A)
Stage Name | SH | (0008,2120)
Stage Number | IS | (0008,2122)
Start Angle | DS | (0054,0200)
Start Cumulative Meterset Weight | DS | (300C,0008)
Start Meterset | DS | (3008,0078)
Start Trim | IS | (0008,2142)
Station Name | SH | (0008,1010)
Steering Angle | FD | (0018,6036)
Stop Trim | IS | (0008,2143)
Storage Media File-set ID | SH | (0088,0130)
Storage Media File-set UID | UI | (0088,0140)
Structure Set Date | DA | (3006,0008)
Structure Set Description | ST | (3006,0006)
Structure Set Label | SH | (3006,0002)
Structure Set Name | LO | (3006,0004)
Structure Set ROI Sequence | SQ | (3006,0020)
Structure Set Time | TM | (3006,0009)
Study Arrival Date | DA | (0032,1040)
Study Arrival Time | TM | (0032,1041)
Study Comments | LT | (0032,4000)
Study Completion Date | DA | (0032,1050)
Study Completion Time | TM | (0032,1051)
Study Component Status ID | CS | (0032,1055)
Study Date | DA | (0008,0020)
Study Description | LO | (0008,1030)
Study ID | SH | (0020,0010)
Study ID Issuer | LO | (0032,0012)
Study Instance UID | UI | (0020,000D)
Study Priority ID | CS | (0032,000C)
Study Read Date | DA | (0032,0034)
Study Read Time | TM | (0032,0035)
Study Status ID | CS | (0032,000A)
Study Time | TM | (0008,0030)
Study Verified Date | DA | (0032,0032)
Study Verified Time | TM | (0032,0033)
Supported Image Display Formats Sequence | SQ | (2000,00A8)
Surface Entry Point | DS | (300A,012E)
Synchronization Channel | US | (0018,106C)
Synchronization Frame of Reference UID | UI | (0020,0200)
Synchronization Trigger | CS | (0018,106A)
Syringe Counts | IS | (0018,1045)
Table Angle | DS | (0018,1138)
Table Height | DS | (0018,1130)
Table Lateral Increment | DS | (0018,1136)
Table Longitudinal Increment | DS | (0018,1137)
Table Motion | CS | (0018,1134)
Table of Parameter Values | FL | (0018,605A)
Table of Pixel Values | UL | (0018,6058)
Table of X Break Points | UL | (0018,6052)
Table of Y Break Points | FD | (0018,6054)
Table Top Eccentric Angle | DS | (300A,0125)
Table Top Eccentric Angle Tolerance | DS | (300A,004E)
Table Top Eccentric Axis Distance | DS | (300A,0124)
Table Top Eccentric Rotation Direction | CS | (300A,0126)
Table Top Lateral Position | DS | (300A,012A)
Table Top Lateral Position Tolerance | DS | (300A,0053)
Table Top Lateral Setup Displacement | DS | (300A,01D6)
Table Top Longitudinal Position | DS | (300A,0129)
Table Top Longitudinal Position Tolerance | DS | (300A,0052)
Table Top Longitudinal Setup Displacement | DS | (300A,01D4)
Table Top Vertical Position | DS | (300A,0128)
Table Top Vertical Position Tolerance | DS | (300A,0051)
Table Top Vertical Setup Displacement | DS | (300A,01D2)
Table Traverse | DS | (0018,1131)
Table Type | CS | (0018,113A)
Table Vertical Increment | DS | (0018,1135)
Target Maximum Dose | DS | (300A,0027)
Target Minimum Dose | DS | (300A,0025)
Target Prescription Dose | DS | (300A,0026)
Target Underdose Volume Fraction | DS | (300A,0028)
Template Extension Creator UID | UI | (0040,DB0D)
Template Extension Flag | CS | (0040,DB0B)
Template Extension Organization UID | UI | (0040,DB0C)
Template Identifier | CS | (0040,DB00)
Template Local Version | DT | (0040,DB07)
Template Name | LO | (300A,0244)
Template Number | IS | (300A,0240)
Template Type | SH | (300A,0242)
Template Version | DT | (0040,DB06)
Temporal Position Identifier | IS | (0020,0100)
Temporal Range Type | CS | (0040,A130)
Temporal Resolution | DS | (0020,0110)
Text Object Sequence | SQ | (0070,0008)
Text String | LO | (2030,0020)
Text Value | UT | (0040,A160)
Therapy Description | CS | (0018,0039)
Therapy Type | CS | (0018,0037)
Thermal Index | DS | (0018,5024)
TID Offset | SS | (0028,6120)
Time | TM | (0040,A122)
Time Distribution Protocol | CS | (0018,1802)
Time of Last Calibration | TM | (0018,1201)
Time of Last Detector Calibration | TM | (0018,700E)
Time of Secondary Capture | TM | (0018,1014)
Time Slice Vector | US | (0054,0100)
Time Slot Information Sequence | SQ | (0054,0072)
Time Slot Time | DS | (0054,0073)
Time Slot Vector | US | (0054,0070)
Time Source | SH | (0018,1801)
Timezone Offset From UTC | SH | (0008,0201)
TM-Line Position X0 | UL | (0018,603C)
TM-Line Position X1 | UL | (0018,6040)
TM-Line Position Y0 | UL | (0018,603E)
TM-Line Position Y1 | UL | (0018,6042)
Tolerance Table Label | SH | (300A,0043)
Tolerance Table Number | IS | (300A,0042)
Tolerance Table Sequence | SQ | (300A,0040)
Tomo Angle | DS | (0018,1470)
Tomo Class | CS | (0018,1491)
Tomo Layer Height | DS | (0018,1460)
Tomo Time | DS | (0018,1480)
Tomo Type | CS | (0018,1490)
Topic Author | LO | (0088,0910)
Topic Key Words | LO | (0088,0912)
Topic Subject | ST | (0088,0906)
Topic Title | LO | (0088,0904)
Total Block Tray Factor | DS | (300A,00F2)
Total Compensator Tray Factor | DS | (300A,00E2)
Total Number of Exposures | US | (0040,0301)
Total Reference Air Kerma | DS | (300A,0250)
Total Time | UL | (50xx,200A)
Total Time of Fluoroscopy | US | (0040,0300)
Transaction UID | UI | (0008,1195)
Transducer Data | LO | (0018,5010)
Transducer Frequency | UL | (0018,6030)
Transducer Orientation Modifier Sequence | SQ | (0008,2246)
Transducer Orientation Sequence | SQ | (0008,2244)
Transducer Position Modifier Sequence | SQ | (0008,2242)
Transducer Position Sequence | SQ | (0008,2240)
Transducer Type | CS | (0018,6031)
Transfer Syntax UID | UI | (0002,0010)
Transfer Tube Length | DS | (300A,02A4)
Transfer Tube Number | IS | (300A,02A2)
Transmitting Coil | SH | (0018,1251)
Transverse Mash | IS | (0054,1202)
Treatment Control Point Date | DA | (3008,0024)
Treatment Control Point Time | TM | (3008,0025)
Treatment Date | DA | (3008,0250)
Treatment Delivery Type | CS | (300A,00CE)
Treatment Intent | CS | (300A,000A)
Treatment Machine Name | SH | (300A,00B2)
Treatment Machine Sequence | SQ | (300A,0206)
Treatment Protocols | LO | (300A,0009)
Treatment Session Application Setup Sequence | SQ | (3008,0110)
Treatment Session Beam Sequence | SQ | (3008,0020)
Treatment Sites | LO | (300A,000B)
Treatment Status Comment | ST | (3008,0202)
Treatment Summary Calculated Dose Reference Sequence | SQ | (3008,0050)
Treatment Summary Measured Dose Reference Sequence | SQ | (3008,00E0)
Treatment Termination Code | SH | (3008,002B)
Treatment Termination Status | CS | (3008,002A)
Treatment Time | TM | (3008,0251)
Treatment Verification Status | CS | (3008,002C)
Trigger Sample Position | UL | (0018,106E)
Trigger Source or Type | LO | (0018,1061)
Trigger Time | DS | (0018,1060)
Trigger Time Offset | DS | (0018,1069)
Trigger Vector | IS | (0054,0210)
Trigger Window | IS | (0018,1094)
Trim | CS | (2010,0140)
Type of Data | CS | (50xx,0020)
Type of Detector Motion | CS | (0054,0202)
Type of Filters | LO | (0018,1161)
UID | UI | (0040,A124)
Ultrasound Color Data Present | US | (0028,0014)
Unformatted Text Value | ST | (0070,0006)
Units | CS | (0054,1001)
Value Type | CS | (0040,A040)
Variable Flip Angle Flag | CS | (0018,1315)
Verification DateTime | DT | (0040,A030)
Verification Flag | CS | (0040,A493)
Verifying Observer Identification Code Sequence | SQ | (0040,A088)
Verifying Observer Name | PN | (0040,A075)
Verifying Observer Sequence | SQ | (0040,A073)
Verifying Organization | LO | (0040,A027)
Vertices of the Polygonal Collimator | IS | (0018,1720)
Vertices of the Polygonal Shutter | IS | (0018,1620)
Video Image Format Acquired | SH | (0018,1022)
View Code Sequence | SQ | (0054,0220)
View Modifier Code Sequence | SQ | (0054,0222)
View Name | SH | (0008,2127)
View Number | IS | (0008,2128)
View Position | CS | (0018,5101)
Visit Comments | LT | (0038,4000)
Visit Status ID | CS | (0038,0008)
VOI LUT Sequence | SQ | (0028,3010)
Waveform Bits Allocated | US | (5400,1004)
Waveform Bits Stored | US | (003A,021A)
Waveform Channel Number | IS | (003A,0202)
Waveform Data | OB or OW | (5400,1010)
Waveform Originality | CS | (003A,0004)
Waveform Padding Value | OB or OW | (5400,100A)
Waveform Sample Interpretation | CS | (5400,1006)
Waveform Sequence | SQ | (5400,0100)
Wedge Angle | IS | (300A,00D5)
Wedge Factor | DS | (300A,00D6)
Wedge ID | SH | (300A,00D4)
Wedge Number | IS | (300A,00D2)
Wedge Orientation | DS | (300A,00D8)
Wedge Position | CS | (300A,0118)
Wedge Position Sequence | SQ | (300A,0116)
Wedge Sequence | SQ | (300A,00D1)
Wedge Type | CS | (300A,00D3)
Whole Body Technique | CS | (0018,1301)
Window Center | DS | (0028,1050)
Window Center & Width Explanation | LO | (0028,1055)
Window Width | DS | (0028,1051)
X Focus Center | DS | (0018,1183)
X offset in Slide Coordinate System | DS | (0040,072A)
X-Ray Image Receptor Angle | DS | (3002,000E)
X-Ray Image Receptor Translation | DS | (3002,000D)
X-Ray Output | DS | (0040,0312)
X-ray Tube Current | IS | (0018,1151)
X-Ray Tube Current in mA | DS | (0018,8151)
Y Focus Center | DS | (0018,1184)
Y offset in Slide Coordinate System | DS | (0040,073A)
Z offset in Slide Coordinate System | DS | (0040,074A)
Zoom Center | DS | (0028,0032)
Zoom Factor | DS | (0028,0031)